areaIntegrator {DIAlignR} | R Documentation

## Calculates area between signal-boundaries.

### Description

This function sums all the intensities between left-index and right-index.

### Usage

    areaIntegrator(l1, leftIdx, rightIdx)

### Arguments

`l1` | (list) A list of vectors. All vectors must be of same length.
`leftIdx` | (numeric) Left index (0-based) of the boundary.
`rightIdx` | (numeric) Right index (0-based) of the boundary.

### Value

area (numeric).

### Author(s)

Shubham Gupta, shubh.gupta@mail.utoronto.ca ORCID: 0000-0003-3500-8152 License: (c) Author (2019) + MIT Date: 2019-03-08

### Examples

    l1 <- list(1:10, 1:10, 1:10)
    areaIntegrator(l1, leftIdx = 4, rightIdx = 6) # 54

[Package DIAlignR version 0.99.12 Index]