layoutPlot {IONiseR} | R Documentation

## Create layout plot of flowcell

### Description

Creates a plot representing the layout of a MinION flow cell. Each circle represents an idividual channel with the intensity relecting the total kilobases of sequence produced. This only considers reads marked as template or complement, 2D reads are ignored as they are generated from the former two.

### Usage

    layoutPlot(summaryData, attribute = NULL)

### Arguments

`summaryData` | Object of class Fast5Summary.
`attribute` | Character string indicating what to plot. Currently accepted values are: "nreads", "kb", "signal".

### Value

Returns an object of `gg` representing the plot.

### Examples

    if( require(minionSummaryData) ) {
       data(s.typhi.rep2, package = 'minionSummaryData')
       layoutPlot( s.typhi.rep2, attribute = 'nreads' )
       layoutPlot( s.typhi.rep2, attribute = 'kb' )
    }

[Package IONiseR version 2.11.0 Index]