gate_tail {openCyto} | R Documentation

## Gates the tail of a density using the derivative of a kernel density estimate

### Description

These methods aim to set a one-dimensional gate (cutpoint) near the edge of a peak in the density specified by a channel of a `flowFrame` to isolate the tail population. They allow two approaches to do this, both beginning by obtaining a smoothened kernel density estimate (KDE) of the original density and then utilizing either its first or second derivative.

### Usage

    gate_tail(fr, channel, filterId = "", num_peaks = 1, ref_peak = 1,
      strict = TRUE, tol = 0.01, side = "right", min = NULL,
      max = NULL, bias = 0, ...)

### Arguments

`fr` | a `flowFrame` object
`channel` | the channel from which the cytokine gate is constructed
`filterId` | the name of the filter
`num_peaks` | the number of peaks expected to see. This effectively removes any peaks that are artifacts of smoothing
`ref_peak` | After `num_peaks` are found, this argument provides the index of the reference population from which a gate will be obtained.
`strict` | `logical` when the actual number of peaks detected is less than `ref_peak`, an error is reported by default. But if `strict` is set to FALSE, then the reference peak will be reset to the peak of the far right.
`tol` | the tolerance value used to construct the cytokine gate from the derivative of the kernel density estimate. See details.
`side` | On which side of the density do we want to gate the tail, the `'right'` (default) or `'left'`?
`min` | a numeric value that sets the lower boundary for data filtering
`max` | a numeric value that sets the upper boundary for data filtering
`bias` | a numeric value that adds a constant to the calculated cutpoint(threshold). Default is 0.
`...` | additional arguments used in calculating derivative. See details.
`method` | the method used to select the cutpoint. Either "first_deriv" or "second_deriv". See details.
`auto_tol` | when TRUE, it tries to set the tolerance automatically. See details.
`adjust` | the scaling adjustment applied to the bandwidth used in the first derivative of the kernel density estimate

### Details

The default behavior of the first approach, specified by `method = "first_deriv"`, finds valleys in the first derivative of the KDE and uses the lowest such valley to place the cutpoint on the steep right shoulder of the largest peak in the original density.

The default behavior of the second approach, specified by `method = "second_deriv"`, is to find peaks in the second derivative of the KDE and use the largest such peak to place the cutpoint at the point on the right shoulder of the largest peak in the original density where it is most rapidly flattening (the first derivative is rapidly growing less negative).

Both approach can be significantly modified from defaults with a number of optional arguments. The `num_peaks` argument specifes how many peaks should be found in the smoothened KDE and `ref_peak` specifies around which peak the gate's cutpoint should be placed (starting from the leftmost peak). Setting the `side` argument to "left" modifies the procedure to put the cutpoint on the left side of the reference peak to isolate a left tail. The `max` and `min` arguments allow for pre-filtering extreme values in the channel of interest (keeping only observations with channel values less than max and/or more than min). The bandwidth used for kernel density estimation can be proportionally scaled using `adjust` (e.g. `adjust = 0.5` will use a bandwidth that is half of the default). This allows for tuning the level of smoothing applied in the estimation.

Lastly, the `tol`, `auto_tol`, and `bias` arguments allow for adjustments to be made to the cutpoint that would otherwise be returned. `tol` provides a tolerance value that the absolute value of the KDE derivative at the cutpoint must be under. If the derivative at the original cutpoint is greater than `tol` in magnitude, the returned cutpoint will be the first point to the right of the original cutpoint (or to the left in the case of `side = "left"`) with corresponding derivative within `tol`. Thus in practice, a smaller value for `tol` effectively pushes the cutpoint further down the shoulder of the peak towards the flat tail. `tol` is set to 0.01 by default but setting `auto_tol = TRUE` will set the tolerance to a reasonable estimate of 1% of the maximum absolute value of the first derivative of the KDE. `tol` and `auto_tol` are only used for `method = "first_deriv"`. Additionally, the `bias` argument allows for directly shifting the returned cutpoint left or right.

It is also possible to pass additional arguments to control the calculation of the derivative, which will have some effect on the resulting cutpoint determination, but this should usually not be needed. By default the number of grid points for the derivative calculation will be 10,000, but this can be changed with `num_points`. The default bandwidth can also be directly adjusted with `bandwidth`, where the final value used will be given by `adjust*bandwidth`

### Value

a `filterList` containing the gates (cutpoints) for each sample with the corresponding `rectangleGate` objects defining the tail as the positive population.

### Examples

    ## Not run:
     gate <- gate_tail(fr, Channel = "APC-A") # fr is a flowFrame

    ## End(Not run)

[Package openCyto version 1.99.2 Index]