correctUnmix {flowSpecs} | R Documentation

## Correct defects in spectral unmixing by compensation

### Description

This function provides a way to reduce the defects in the spectral unmixing, by creating a secondary correction matrix, which is symmetrical.

### Usage

    correctUnmix(unmixFlowObj, corrMat, transCoFacs = 400)

### Arguments

`unmixFlowObj` | A flowframe or flowset post unmixing.
`corrMat` | A correction matrix. If this is the first round, the executionof this function needs to be preceeded by the generation of this matrix, for example by using the `corrMatCreate` function.
`transCoFacs` | If transformation should be performed, the transformation cofactors can be added here. Three possible inputs: a vector with specific cofactors for each variable, a set value that will be used for all variables, and FALSE. Note: It might be good to set this to FALSE in the final round, to optimize the transoformations externally.

### Value

The unmixed flow object, now corrected with the values from the corrMat.

### See Also

`specUnmix`, `arcTrans`, `corrMatCreate`

### Examples

    # Load uncompensated data
    data(fullPanel)

    # Load the spectral unmixing matrix generated with controls from the same
    # experiment. These can be generated using the specMatCalc function.
    data(specMat)

    # And now unmix
    fullPanelUnmix <- specUnmix(fullPanel, specMat)

    # Create an empty unmixinng matrix
    corrMat <- corrMatCreate(specMat)

    # Now correct the data with this. In the first instance, this will of course
    # not have any effect, more  than transformation, as the corrMat is empty.
    fullPanelCorr <- correctUnmix(fullPanelUnmix, corrMat)

    # This now needs to be investigated, to identify any possible compensation
    # defects. This is most easily done with the oneVsAllPlot executed in the
    # following way:
    ## Not run:
    oneVsAllPlot(fullPanelCorr)

    ## End(Not run)
    # One obvoius defect that shows when doing this is between CD56 and IgM:
    oneVsAllPlot(fullPanelCorr, "BV650_CD56", saveResult = FALSE)

    # This is corrcted the following way:
    corrMat["BV650_CD56", "AF647_IgM"] <- -0.03
    fullPanelCorr <- correctUnmix(fullPanelUnmix, corrMat)
    oneVsAllPlot(fullPanelCorr, "BV650_CD56", saveResult = FALSE)

    # This process is iterated until there are no remaining artifacts. Good help
    # to do this is a set of fluorescence-minus-one controls. If that is not
    # available, a rule of thumb is that if the signal in marker x is
    # strongly negatively correlated to marker y, so that highly
    # single-x-posisive values are below zero, then this is with all likelihood
    # an artifact. The situation becomes more complicated with strong positive
    # correlations, as they can occur in biology, so there one has to take more
    # care and keep the marker biology in mind.

[Package flowSpecs version 1.6.0 Index]